Draw graphics for the game either by hand or on computer

Print out and/or cut out graphics for game.

Use spray adhesive to glue graphics onto cardboard

Punch holes for ‘ball catchers’

Use spray adhesive to glue graphics onto MDF base

Measure outside walls and mark to correct length

Saw outside walls with Tenon Saw to length

Use PVA adhesive to glue outside walls onto base

Measure and mark inside walls to length

Saw inside walls with Tenon Saw to desired length.

Lightly sand inside walls.

Use PVA adhesive to glue inside walls onto base

Allow 1 hour for PVA adhesive to dry.

Measure and mark screw holes in clear acrylic top.

Drill screw holes.

Counter sink screw holes.

Add balls to game.

Screw down acrylic top with 2mm Philip head screws.

Sand down edges of the game on the Disk Sander.

Hand-sand any sharp edges of your game.

Play!